1. 512 kb
2. 128 kb
3. 80 Mhz
4. SFR
5. F0 should output low to turn on the LED. D7 will output high when the User button is not pressed.